**100 kVA/80 kW UPS POWER POD**



**100 kVA UPS Power POD**

* + - **Input & Output Switchgear**
		- **Pre-wired: Input & Output Cam Locks**
		- **N+1 HVAC: Cooling Redundancy**

|  |  |
| --- | --- |
| **UPS INFORMATION** |   |
| Manufacturer | Mitsubishi  |
| Series/Model | 9700 Series Model 150 |
| Rating kVA KW | 100 kVA / 80 KW  |
| Input Voltage | 480V 4W +G |
| Input Wiring (required on site) |  (2) Set 4/0 Cam Lock Connections |
| Output Voltage | 480V 4W +G |
| Output Wiring (required on site) |  (2) Set 4/0 Cam Lock Connections |
| Wrap-Around Maintenance Bypass | With Kirk Key and Solenoid Key Release |
| **UPS BATTERY INFORMATION** |   |
| Battery Type | Enersys HX 12-400 |
| Estimated Battery Run-Time | 8 Minutes (Standard) – extended runtime options are available. |
| **HVAC INFORMATION** |   |
| Manufacturer | AirSys |
| Number of A/C Units | 2 |
| Tonnage Capacity: Per Unit | 4 Ton |
| Total Tonnage Capacity | 8 Ton |